|  |
| --- |
| #include “Ultrasonic.h" |
|  | Ultrasonic ultrasonic(6,2); |
|  | int distance; void setup() |
|  | { |
|  | Serial.begin(9600); |
|  | } |
|  | void loop() { |
|  | distance = ultrasonic.read(CM); Serial.print("Distance |
|  | in CM: “); |
|  | Date 30th October 2022 |
|  | Team ID PNT2022TMID23663 |
|  | Roll No 612919104054 |
|  | Project Name Project:- Signs With Smart Connectivity For Better |
|  | Safety |
|  | Serial.println(distance); if |
|  | (distance < 100) |
|  | Serial.print("alert"); |
|  | Serial.println(); delay(3000); |
|  | } |